|  |  |
| --- | --- |
|  ITEM NO.: 6096 - REMCO | **ASSEMBLY INSTRUCTIONS** |
| Step 1 Step 2 Step 3 | **Carefully unpack all parts before attempting to assemble.** |
| 1. Tilt the back cushion to the appropriate angle and then fasten it with the two bolts (B), see ‘a-a’ on the left for a detailed picture.
2. Fit the seat frame (A) to the upright post on the base (C).
3. Assembly finished.

 |
| **PARTS LIST** |
| **A –Seat Frame** | **1** |
| **B–Bolt** | **2** |
| **C—Base** | **1** |
|  |  |
|  |  |

|  |  |
| --- | --- |
|  ITEM NO.: 6096 - REMCO (FOOTSTOOL)  | **ASSEMBLY INSTRUCTIONS** |
|  | **Carefully unpack all parts before attempting to assemble.** |
| 1. Place the footstool top (A) onto the post (B) and fix with screws (D). Tighten the screws well using the wrench (F).
2. Take the screws (E – M8x50) and slide a washer (H) onto it. Use these to fix the post (B) onto the base (C). Tighten the screws well using the wrench (G).
3. Assembly finished.
 |
| **PARTS LIST** |
| **A –Footstool Top** | **1** |
| **B– Post** | **1** |
| **C – Base** | **1** |
| **D—Screw（M6X20）** | **4** |
| **E—Screw（M8X50）** | **3** |
| **F—Wrench for M6 Screw** | **1** |
| **G—Wrench for M8 Screw** | **1** |
| **H—Washer** | **3** |

Step 1

Step 2