|  |  |  |
| --- | --- | --- |
| ITEM NO.: 6101 - OHIO | **ASSEMBLY INSTRUCTIONS** | |
|  | **Carefully unpack all parts before attempting to assemble.** | |
| 1. Tilt the back cushion to the appropriate angle and then fasten it with the two bolts (B), see detailed picture on the left. 2. Fix each armrest in place with two bolts (D) and a washer (E). Tighten with wrench. 3. Fit the chair body (A) to the upright post on the base (C). 4. Assembly finished. | |
| **PARTS LIST** | |
| **A – Chair body** | **1** |
| **B - Bolt** | **2** |
| **C - Base** | **1** |
| **D - Socket Head Bolt (M6\*55\*Head diameter \*10mm)** | **4** |
| **E - Washer (6mm\*13mm\*1.5mm)** | **4** |
|  |  |

|  |  |  |
| --- | --- | --- |
| ITEM NO.: 6101 - OHIO (FOOTSTOOL) | **ASSEMBLY INSTRUCTIONS** | |
|  | **Carefully unpack all parts before attempting to assemble.** | |
| 1. Place the footstool top (A) onto the post (B) and fix with screws (D). Tighten the screws well using the wrench (F). 2. Take one of the screws (E) and slide a washer (H) onto it.  Repeat for the other screws and use these to fix the metal post (B) onto the base (C). Tighten the screws well using the wrench (G). 3. Assembly finished. | |
| **PARTS LIST** | |
| **A - Footstool Top** | **1** |
| **B - Post** | **1** |
| **C - Base** | **1** |
| **D - Screw（M6X20）** | **4** |
| **E - Screw（M8X50）** | **3** |
| **F - Wrench for M6 Screw** | **1** |
| **G - Wrench for M8 Screw** | **1** |
| **H - Washer** | **3** |