|  |  |
| --- | --- |
|  ITEM NO.: 6226 – KD Chair | **ASSEMBLY INSTRUCTIONS** |
|  | **Carefully unpack all parts before attempting to assemble.** |
| 1. Place the metal frame (A) onto the designated place on the seat cushion (B) then fix with cross screws (D).
2. Repeat step 1 on the other side.
3. Insert the iron tube on the back cushion (C) into the corresponding tube on the seat frame (B); ensure both sides are pushed down evenly.
4. Insert the inner hexagon screw (E) into the hole at the bottom of the seat cushion (B) and tighten it with the wrench (F).
5. Repeat step 4 on the other side.
6. Assembly finished.
 |
| **PARTS LIST** |
| **A - Metal frame** | **2** |
| **B - Seat cushion** | **1** |
| **C - Back cushion** | **1** |
| **D - Cross screw** | **8** |
| **E - Screw** | **2** |
| **F—**[**Wrench**](http://www.youdao.com/w/internal%20hexagonal%20wrench/#keyfrom=E2Ctranslation) | **1** |