|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| ITEM NO.: 8183 - ARHUS | **ASSEMBLY INSTRUCTION** | | | |
|  | **Carefully unpack all parts before attempting to assemble.** | | | |
| **PARTS LIST** | | | |
| **DIAGRAM** | **PART NAME** | **SIZE** | **QTY** |
|  | **A-Headboard** |  | **1** |
|  | **B-Box Spring** |  | **2** |
|  | **C-Feet for Box spring** | **60\*60\*160mm** | **8** |
|  | **D-Metal Feet** | **60\*60\*95mm** | **2** |
|  | **E-Hook** |  | **2** |
|  | **F- KD Crocodile clip** |  | **1** |
|  | **G-Screw of Metal feet** | **M5\*30MM\*Head Dia\*10mm** | **8** |
|  | **H-Screw of KD Crocodile clip** | **M4\*30mm** | **10** |
| 1. Fix the feet (C) into the base of the boxsprings (B). See detailed picture for positioning. 2. Fix the two feet (D) into the base of the boxsprings using screws (G). 3. Connect the two boxsprings together by fixing the K/D crocodile clip (F) in place using screws (I), then connect the two parts of the K/D crocodile clip (F). 4. Slot the two pairs of hooks (E) on the headboard (A) into their corresponding pair of hooks on the boxspring (B). 5. Assembly finished. | | | |