|  |  |
| --- | --- |
| ITEM NO.: 8121 - PICARDIE | **ASSEMBLY INSTRUCTION** |
|  | **Carefully unpack all parts before attempting to assemble.** |
| **PARTS LIST** |
| **DIAGRAM** | **PART NAME** | **SIZE** | **QTY** |
|  | **A - Headboard** |  | **1** |
|  | **B - Boxspring** |  | **2** |
|  | **C - Feet** | **60\*60\*160mm** | **8** |
|  | **D - K/D crocodile clip** |  | **1** |
|  | **E - Screw** | **M4\*30mm** | **10** |
|  |  |  |  |
| 1. Fix the wooden feet (C) into the base of the boxsprings (B). See detailed picture for positioning.
2. Connect the two boxsprings together by fixing the K/D crocodile clip (D) in place using screws (E), then connect the two parts of the K/D crocodile clip (D).
3. Slot the two pairs of hooks on the headboard (A) into their corresponding pair of hooks on the boxspring (B).
4. Assembly finished.
 |