|  |  |
| --- | --- |
| ITEM NO.: 8132 - BRANDON  | **ASSEMBLY INSTRUCTIONS** |
|  | **Carefully unpack all parts before attempting to assemble.** |
| **PARTS LIST** |
|  | **PART NAME** | **SIZE** | **QTY** |
| **A** | **Headboard** |  | **1** |
| **B** | **Box Spring** |  | **2** |
| **C** | **Wooden Feet** | **60\*60\*90mm** | **8** |
| **D** | **Hook** |  | **2** |
| **E** | **K/D Crocodile Clip** |  | **1** |
| **F** | **Screw** | **M4X30mm** | **10** |
|  |  |  |  |
| 1. Fix the wooden feet (C) into the base of the boxsprings (B). See picture for positioning.
2. Connect the two boxsprings together by fixing the K/D crocodile clip (E) in place using screws (F), then connect the two parts of the K/D crocodile clip (E).
3. Slot the two pairs of hooks (D) on the headboard (A) into their corresponding pair of hooks on the boxspring (B).
4. Assembly finished.
 |

|  |  |
| --- | --- |
| ITEM NO.: 8132 BRANDON (SINGLE) | **ASSEMBLY INSTRUCTIONS** |
|  | **Carefully unpack all parts before attempting to assemble.** |
| **PARTS LIST** |
|  | **PART NAME** | **SIZE** | **QTY** |
| **A** | **Headboard** |  | **1** |
| **B** | **Boxspring** |  | **1** |
| **C** | **Feet** | **60\*60\*90mm** | **4** |
| **D** | **Hook** |  | **2** |
| **E** | **Middle foot** | **60\*60\*70MM** | **1** |
|  |  |  |  |
|  |  |  |  |
| 1. Fix the feet (C) and the middle foot (E) into the base of the boxspring (B), see detailed picture for positioning.
2. Slot the two pairs of hooks (D) on the headboard (A) into their corresponding pair of hooks on the boxspring (B).
3. Assembly finished.
 |