|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| ITEM NO.: 8165 - PORT-BAY | **ASSEMBLY INSTRUCTIONS** | | | |
|  | **Carefully unpack all parts before attempting to assemble.** | | | |
| **PARTS LIST** | | | |
| **DIAGRAM** | **PART NAME** | **SIZE** | **QTY** |
|  | **A - Headboard** |  | **1** |
|  | **B - Boxspring** |  | **2** |
|  | **C - Feet** | **60\*60\*160mm** | **8** |
|  | **D - Hook** |  | **2** |
|  | **E - K/D Crocodile Clip** |  | **1** |
|  | **F - Screw for K/D Crocodile Clip** | **M4\*30mm** | **10** |
|  |  |  |  |
| 1. Fix the feet (C) into the base of the boxsprings (B). See detailed picture for positioning. 2. Connect the two boxsprings together by fixing the K/D crocodile clip (E) in place using screws (F), then connect the two parts. 3. Slot the two pairs of hooks (D) on the headboard (A) into their corresponding pair of hooks on the boxspring (B). 4. Assembly finished. | | | |