|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| ITEM NO.: 8176 - KOPENHAGEN | **ASSEMBLY INSTRUCTIONS** | | | |
|  | **Carefully unpack all parts before attempting to assemble.** | | | |
| **PARTS LIST** | | | |
| **DIAGRAM** | **PART NAME** | **SIZE** | **QTY** |
|  | **A - Headboard** |  | **1** |
|  | **B - Boxspring** |  | **2** |
|  | **C - Feet for Box spring** | **60\*60\*160mm** | **8** |
|  | **D – Round feet** | **60\*60\*140mm** | **2** |
|  | **E - Hook** |  | **2** |
|  | **F - KD Crocodile clip** |  | **1** |
|  | **G - Screw for K/D crocodile clip** | **M4\*30mm** | **10** |
|  |  |  |  |
| 1. Fix the feet (C) into the base of the boxsprings (B). See detailed picture for positioning. 2. Fix the two feet (D) into the base of the boxsprings (B). 3. Connect the two boxsprings together by fixing the K/D crocodile clip (F) in place using screws (G), then connect the two parts of the clip (F). 4. Slot the two pairs of hooks (E) on the headboard (A) into the hooks on the boxspring. 5. Assembly finished. | | | |