|  |  |
| --- | --- |
| ITEM NO.: 8177 - SABINE | **ASSEMBLY INSTRUCTIONS** |
|  | **PARTS LIST** |
|  | **PART NAME** | **SIZE** | **QTY** |
| **A** | **Headboard** |  | **1** |
| **B** | **Boxspring** |  | **2** |
| **C** | **Feet** | **60\*60\*160mm** | **8** |
| **D** | **Hook** |  | **4** |
| **E** | **Footboard** |  | **1** |
|  |  |  |  |
|  |  |  |  |
| 1. Fix the feet (C) to the base of the boxspring (B), see detailed picture for positioning.
2. Slot the two pairs of hooks (D) on the headboard (A) into their corresponding pair of hooks on the boxspring (B).
3. Repeat step two for the footboard (E).
4. Assembly finished.
 |

|  |  |
| --- | --- |
| ITEM NO.: 8177 - SABINE (1.4m)  | **ASSEMBLY INSTRUCTIONS** |
|  | **PARTS LIST** |
|  | **PART NAME** | **SIZE** | **QTY** |
| **A** | **Headboard** |  | **1** |
| **B** | **Boxspring** |  | **1** |
| **C** | **Wooden Feet** | **60\*60\*160mm** | **4** |
| **D** | **Hook** |  | **4** |
| **E** | **Middle Foot** | **60\*60\*140mm** | **1** |
| **F** | **Footboard** |  | **1** |
|  |  |  |  |
| 1. Fix the feet (C) and the middle foot (E) into the base of the boxspring (B), see detailed picture for positioning.
2. Slot the two pairs of hooks (D) on the headboard (A) into their corresponding pair of hooks on the boxspring (B).
3. Repeat step two for the footboard (F).
4. Assembly finished.

 |