|  |  |
| --- | --- |
| ITEM NO.: 8185 - PRESTON | **ASSEMBLY INSTRUCTION** |
|  | **Carefully unpack all parts before attempting to assemble.** |
| **PARTS LIST** |
| **DIAGRAM** | **PART NAME** | **SIZE** | **QTY** |
|  | **A-Headboard** |  | **1** |
|  | **B-Box spring** |  | **2** |
|  | **C-Feet** | **60\*60\*90mm** | **8** |
|  | **D-Feet** |  | **2** |
|  | **E-Hook** |  | **2** |
|  | **F-KD Crocodile Clip** |  | **1** |
|  | **G- Screw for KD Crocodile Clip** | **M4\*30mm** | **10** |
|  | **H-Screw for Feet (D)** | **M5\*45\*Head Dia. \*10mm** | **8** |
| 1. Fix the feet (C) into the base of the boxsprings (B). See detailed picture for positioning.
2. Fix the two corner-shaped feet (D) into the base of the boxsprings using screws (H).
3. Connect the two boxsprings together by fixing the K/D crocodile clip (F) in place using screws (G), then connect the two parts of the K/D crocodile clip (F).
4. Slot the two pairs of hooks (E) on the headboard (A) into their corresponding pair of hooks on the boxspring (B).
5. Assembly finished.
 |