|  |  |
| --- | --- |
| ITEM NO.: 8198 - MONTENEGRO | **ASSEMBLY INSTRUCTION** |
|  | **Carefully unpack all parts before attempting to assemble.** |
| **PARTS LIST** |
| **DIAGRAM** | **PART NAME** | **SIZE** | **QTY** |
|  | **A - Headboard** |  | **1** |
|  | **B - Boxspring** |  | **2** |
|  | **C - Wooden feet** | **60\*60\*160mm** | **8** |
|  | **D - Hook** |  | **2** |
|  | **E - KD Crocodile Clip** |  | **1** |
|  | **F - Screw** | **M4\*30mm** | **10** |
| 1. Fix the wooden feet (C) into the base of the boxsprings (B). See detailed picture for positioning.
2. Connect the two boxsprings together by fixing the K/D crocodile clip (E) in place using screws (F), then connect the two parts of the K/D crocodile clip (E).
3. Slot the two pairs of hooks (D) on the headboard (A) into the corresponding pair of hooks on the boxspring.
4. Assembly finished.
 |