|  |  |  |  |
| --- | --- | --- | --- |
| ITEM NO.: 8316 - ALBY | **ASSEMBLY INSTRUCTIONS** | | |
|  | **Carefully unpack all parts before attempting to assemble.** | | |
| 1. Fix the feet (C) into the base of the boxsprings (B). See detailed picture for positioning. 2. Connect the two boxsprings together by fixing the K/D crocodile clip (E) in place using screws (F), then connect the two parts of the K/D crocodile clip (E). 3. Slot the two pairs of hooks (D) on the headboard (A) into their corresponding pair of hooks on the boxspring (B). 4. Assembly finished. | | |
| **PARTS LIST** | | |
| **A – Headboard** |  | **1** |
| **B – Boxspring** |  | **2** |
| **C – Feet** |  | **8** |
| **D – Hook** |  | **2** |
| **E – K/D crocodile clip** |  | **1** |
| **F – Screw** |  | **10** |