|  |  |
| --- | --- |
| ITEM NO.: 8323 - LEXINGTON | **ASSEMBLY INSTRUCTIONS** |
|  | **Carefully unpack all parts before attempting to assemble.** |
| 1. Fix the feet (C) onto the base of the boxsprings (B).
2. Connect the two boxsprings together by fixing the K/D crocodile clip (E) in place using screws (F), then connect the two parts.
3. Slot the two pairs of hooks (D) on the headboard (A) into their corresponding pair of hooks on the boxspring (B).
4. Assembly finished.
 |
| **PARTS LIST** |
| **A–Headboard** |  | **1** |
| **B–Boxspring** |  | **2** |
| **C–Feet** |  | **8** |
| **D–Hook** |  | **2** |
| **E– KD Crocodile Clip** |  | **1** |
| **F–Screw** |  | **10** |