|  |  |
| --- | --- |
|  ITEM NO.: 9350 - MADISON | **ASSEMBLY INSTRUCTIONS** |
|  | **Carefully unpack all parts before attempting to assemble.** |
| 1. Fix the metal feet (B) to the corresponding place on the base of the seat (A) using screws (C). Four screws are needed for each corner. Tighten all screws well.
2. Assembly finished.
 |
| **PARTS LIST** |
| **A—Seat** | **1** |
| **B­­—Metal Feet** | **2** |
| **C—Screw** | **16** |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |