|  |  |  |  |
| --- | --- | --- | --- |
| ITEM NO.: 9356 – ROMANO (S2) | **ASSEMBLY INSTRUCTIONS** | | |
|  | **Carefully unpack all parts before attempting to assemble.** | | |
| 1. Fix the wooden feet (A) to the four corners on the base of the sofa, using screws (B). Tighten all screws well. 2. Assembly finished. | | |
| **PARTS LIST** | | |
| **A –Wooden feet** | **102\*102 \*147mm** | **4** |
| **B –Screw** | **M5\*60\*10mm** | **8** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| ITEM NO.: 9356 – ROMANO (S3) | **ASSEMBLY INSTRUCTIONS** | | |
|  | **Carefully unpack all parts before attempting to assemble.** | | |
| 1. Fix the wooden feet (A) to the four corners on the base of the sofa, using screws (B). Tighten all screws well. 2. Fix the middle foot (C) in place using screws (D). Tighten all screws well. 3. Assembly finished. | | |
| **PARTS LIST** | | |
| **A – Wooden Feet** | **102\*102 \*147mm** | **4** |
| **B – Screw** | **M5\*60\*10mm** | **8** |
| **C - Middle Foot** | **100\*32\*147mm** | **1** |
| **D - Screw** | **M5\*30\*10mm** | **4** |
|  |  |  |
|  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| ITEM NO.: 9356 – ROMANO | **ASSEMBLY INSTRUCTIONS** | | |
| D | **Carefully unpack all parts before attempting to assemble.** | | |
| 1. Fix the two long feet (A) and the L-shape feet (B) to their corresponding places on the base of the sofa, using screws (C). Tighten all screws well. 2. Fix the two middle feet (D) to their places on the base of the sofa, using screws (E). 3. Bring the pieces of the sofa together and connect them using the two K/D crocodile clips (F). 4. Assembly finished. | | |
| **PARTS LIST** | | |
| **A –Feet** | **920\*150 \*150mm** | **2** |
| **B –L shape Feet** | **M5\*45\*Head Dia. 10mm** | **4** |
| **C-Screw** | **M5\*60\* Head Dia. 10mm** | **32** |
| **D-Middle Feet** | **150\*150\*150mm** | **2** |
| **E-Screw** | **M5\*30\* Head Dia.10mm** | **8** |
| **F- K/D Clip** |  | **2** |
|  |  |  |