|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| ITEM NO.: 8151 - TOULON | **ASSEMBLY INSTRUCTION** | | | |
|  | **PARTS LIST** | | | |
|  | **PART NAME** | **SIZE** | **QTY** |
| **A** | **Headboard** |  | **1** |
| **B** | **Boxspring** |  | **2** |
| **C** | **Feet** | **60\*60\*160mm** | **8** |
| **D** | **Hook** |  | **2** |
| **E** | **K/D Crocodile Clip** |  | **1** |
| **F** | **Screw** | **M4\*30MM** | **10** |
| 1. Fix the feet (C) into the base of the boxsprings (B). See detailed picture for positioning. 2. Connect the two boxsprings together by fixing the K/D crocodile clip (E) in place using screws (F), then connect the two parts of the K/D crocodile clip (E). 3. Slot the two pairs of hooks (D) on the headboard (A) into their corresponding pair of hooks on the boxspring (B). 4. Assembly finished. | | | |