|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| ITEM NO.: 8207 - STRASBOURG | **ASSEMBLY INSTRUCTIONS** | | | |
|  | **Carefully unpack all parts before attempting to assemble.** | | | |
| **PARTS LIST** | | | |
| **DIAGRAM** | **PART NAME** | **SIZE** | **QTY** |
|  | **A-Headboard** |  | **1** |
|  | **B-Footboard** |  | **1** |
|  | **C-Boxspring** |  | **2** |
|  | **D-Feet** | **60\*60\*160mm** | **8** |
|  | **E-Hook** |  | **4** |
|  |  |  |  |
| 1. Fix the feet (D) into the base of the boxsprings (C). 2. Slot the two pairs of hooks (E) on the headboard (A) into their corresponding pair of hooks on the boxspring (C). 3. Repeat step two for the footboard (B). 4. Assembly finished. | | | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| ITEM NO.：8207 STRASBOURG（EBSB） | **ASSEMBLY INSTRUCTIONS** | | | |
|  | **Carefully unpack all parts before attempting to assemble.** | | | |
| 1. Fix the feet (A) to the base of the boxspring. 2. Open the cover (C) of the motor (B), and fix the motor onto the hook at the bottom of the bed as shown. 3. Lock the motor covers in place by sliding them back on top of the motor. 4. Fix the connecting rods (E) onto the box spring frame with screws (D). | | | |
| **PARTS LIST** | | | |
| **A – Wooden feet** | |  | **8** |
| **B – Motor** | |  | **2** |
| **C – Motor cover** | |  | **2** |
| **D – Screw（1/4”x1.5”）** | |  | **8** |
| **E – Connection rod** | |  | **2** |
|  | |  |  |
|  | |  |  |
|  | |  |  |
| ITEM NO.：8207 STRASBOURG（EBSB） | **ASSEMBLY INSTRUCTIONS** | | | |
|  | **Carefully unpack all parts before attempting to assemble.** | | | |
| 1. Slot the two pairs of hooks (H) on the headboard (F) and footboard (G) into their corresponding pair of hooks on the boxspring (I). 2. Assembly finished. | | | |
| **PARTS LIST** | | | |
| **F – Headboard** |  | | **1** |
| **G – Headboard** |  | | **1** |
| **H – Hook** |  | | **4** |
| **I – Boxspring** |  | | **2** |